Page 138 of 346 Start Back Next End ZBasic System Library 126 ZBasic Microcontrollers Get1WireByte Type Function returning Byte Invocation Get1WireByte(pin) Parameter Method Type Description pin ByVal Byte The pin to be used for 1-Wire I/O. Discussion This function reads a byte value (LSB first) using the 1-Wire protocol. It may be used instead of a series of calls to Get1Wire() in order to read a byte at a time. To perform a 1-Wire operation, this function along with related 1-Wire routines must be used in the proper sequence. See the specifications of your 1- Wire device for more information. Resource Usage This routine uses the I/O Timer and disables interrupts for about 100µS for each bit received. Example Dim b as Byte b = Get1WireByte(12) Compatibility This routine is not available in BasicX compatibility mode. See Also Get1Wire, Get1WireData, Put1Wire, Put1WireByte, Put1WireData, Reset1Wire